,Wattage Comments##OTHER##,WEIGHT##MASS##KILOGRAMS,WATTAGE##ELECTRICAL_WATTAGE##WATTS,VOLTAGE RANGE V##OTHER##,VOLTAGE COMMENTS##OTHER##,VOLTAGE##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,TOTAL HEIGHT##LENGTH##MILLIMETERS,TECHNICAL SHEET##OTHER##,STRUCTURE MATERIAL##OTHER##,ROTATION##ANGLE##DECIMAL DEGREES,RADIUS##LENGTH##MILLIMETERS,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,ON TRACK_OFFSET##LENGTH##MILLIMETERS,ON TRACK##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,LIGHTING MATERIAL##OTHER##,FREQUENCY RANGE Hz##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,DIAMETER##LENGTH##MILLIMETERS,COLOR RENDERING INDEX##OTHER##,COLLECTION##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,AVAILABLE FINISHES##OTHER##,ASSEMBLY SHEET##OTHER##,ACCESSORY CODE##OTHER##,ACCESSORIES##OTHER##
OnCeiling_COB-LED_11W_2700K_664lm_45°,,1.700000000000,11.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,400.000000000000,https://www.luceplan.com/products/e06-wall,LUCEPLAN_ALUMINIUM_MATT-BLACK,180.000000000000,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-extruded-aluminium-ceiling-lamp-e06_349388,1E0600100001+1E060/1M0000,0.000000000000,0,E06100+E061M,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,50/60Hz,Ceiling lights produced in two diameters (70 mm and 134 mm) and various lengths. The recessed positioning of the light source increases the angle of shading and lighting comfort.,0.000000000000,70.000000000000,90,E06,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E060I0005-plafone-bin.pdf,,
OnTrack_COB-LED_11W_2700K_664lm_45°,,1.800000000000,11.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,400.000000000000,https://www.luceplan.com/products/e06-wall,LUCEPLAN_ALUMINIUM_MATT-BLACK,180.000000000000,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-extruded-aluminium-ceiling-lamp-e06_349388,1E0600150001+1E060/1M0000,49.000000000000,1,E06150+E061M,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,50/60Hz,Ceiling lights produced in two diameters (70 mm and 134 mm) and various lengths. The recessed positioning of the light source increases the angle of shading and lighting comfort.,0.000000000000,70.000000000000,90,E06,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E060I0005-plafone-bin.pdf,,
